**Hurry Doctor**

**Changes in original code:**

Original code was for 2 players, New code is for 4 players

**Changes in surgery:**

**Inner child** is replaced by **Broken heart**

**Radial fracture** is replaced by **Writer’s cramp**

**Hopeless case** is replaced by **Water on the knee**

**Mental block** is replaced by **Bread Box**

Changes in Circuit connections:

Pin **A4/19** connection is replaced by **D3/3**

OLED connections:

**VCC** of OLED is connected to **5v** of Arduino Nano

**GND** of OLED is connected to **GND** of Arduino Nano

**SDA** of OLED is connected to **A4/18** of Arduino Nano

**SCL** of OLED is connected to **A5/19** of Arduino Nano

Add OLED Library:

Library is provided with code

Extract file **Adafruit\_SSD1306-master.zip** and copy the folder to library folder of Arduino

You can find library folder where you installed Arduino software

*(e.g. D:\Softwares\Arduino\libraries)*

Restart Arduino IDE after copying